**DS-K1T341A Series MinMoe Terminal**

**Release Notes (2021-12-10)**

|  |  |  |
| --- | --- | --- |
| **Device Model:**  DS-K1T341AM  DS-K1T341AMF  **Naming Rule:**  M for M1 card, F for fingerprint | Firmware Version | ARM: ACS\_641\_AI3\_EN\_STD\_V3.2.30\_build211122  ACS\_641\_AI3\_EN\_NEU\_V3.2.30\_build211122 |
| SDK | Latest version |
| iVMS-4200 Client Version | Latest version baseline |

**Reason of Upgrade**

Fix bugs, enhance products quality and meet customers’ requirements.

**Modified Features**

1. Compatible with new fingerprint module
2. Optimize ISAPI protocol related functions

**DS-K1T341A Series MinMoe Terminal**

**Release Notes (2021-11-15)**

|  |  |  |
| --- | --- | --- |
| **Device Model:**  DS-K1T341AM  DS-K1T341AMF  **Naming Rule:**  M for M1 card, F for fingerprint | Firmware Version | ARM: ACS\_641\_AI3\_EN\_STD\_V3.2.30\_build211110  ACS\_641\_AI3\_EN\_NEU\_V3.2.30\_build211110 |
| SDK | Latest version |
| iVMS-4200 Client Version | Latest version baseline |

**Reason of Upgrade**

Fix bugs, enhance products quality and meet customers’ requirements.

**Modified Features**

1. Fix the device offline issue caused by searching device event from iVMS4200 client through ISUP5.0 protocol;
2. Fixed some issues about ISAPI protocol.
3. Optimize the connection with HikCentral Professional platform;

**DS-K1T341A Series MinMoe Terminal**

**Release Notes (2021-10-18)**

|  |  |  |
| --- | --- | --- |
| **Device Model:**  DS-K1T341AM  DS-K1T341AMF  **Naming Rule:**  M for M1 card, F for fingerprint | Firmware Version | ARM: ACS\_641\_AI3\_EN\_STD\_V3.2.30\_build210731  ACS\_641\_AI3\_EN\_NEU\_V3.2.30\_build210731 |
| SDK | Latest version |
| iVMS-4200 Client Version | Latest version baseline |


**Reason of Upgrade**

Add new function, fix bugs, enhance products quality and meet customers’ requirements.

**New Features**

1. Add Hik-Connect menu in device UI Menu🡪Comm. The function is disabled in default.

图形用户界面, 应用程序

描述已自动生成

**Modified Features**

1. Optimize the wake-up distance of the device screen through the face, and the wake-up distance is consistent with the recognition distance

图形用户界面, 应用程序

描述已自动生成

**DS-K1T341A Series MinMoe Terminal**

**Release Notes (2021-06-23)**

|  |  |  |
| --- | --- | --- |
| **Device Model:**  DS-K1T341AM  DS-K1T341AMF  **Naming Rule:**  M for M1 card, F for fingerprint | Firmware Version | ARM: ACS\_641\_AI3\_EN\_STD\_V3.2.30\_build210609  ACS\_641\_AI3\_EN\_NEU\_V3.2.30\_build210609 |
| SDK | Latest version |
| iVMS-4200 Client Version | Latest version baseline |

**Reason of Upgrade**

Fix bugs, enhance products quality and meet customers’ requirements.

**Modified Features**

1. Optimize the function of exporting data to U disk.
2. Optimize the working mechanism of infrared supplement light.

**Customer Impact and Recommended Action**

This update refers to function/compatibility improvement and will take effect automatically after the Date of Change. We are very sorry for any inconvenience of use-habit changes caused by this action.

For any questions and request for this firmware, please contact our local technical support team.

Note:

* Hikvision reserves the right to change, alter or withdraw the above notification without prior notice.
* Product design and specifications are subject to change without prior notice.
* The Hikvision firmware may contain errors known as errata, which may cause the product to deviate from published specifications. Current characterized errata are available on request.
* Hikvision is not liable for any typing or printing errors.

Hikvision Digital Technology CO., Ltd.

No. 555 Qianmo Road, Binjiang District, Hangzhou 310051, China

Tel: +86-571-8807-5998

FAX: +86-571-8993-5635

Email: overseabusiness@hikvision.com