

1. **Do Not reboot the device after importing the model file. Reboot the device after upgrading the upgrade firmware file.**



1. **Import and upgrade the firmware, then reboot the device**
2. **Import model file, do not reboot the device**
3. **Configure DYNDNS**

****

**Configure according to actual parameters**

**Note: Turning on and off DDNS requires Rebooting the device**

**Model file: ALG\_V2.2.0\_200604**

**Firmware file: DZP20210203131\_tcm403\_a\_EN\_STD\_4.2.5\_210204**