 
Version	Description				   
V1.0	
	·	Initial Beta release, functional			   
						   
V1.0.1	
	·	Added DRO error checks 			   
	·	Auto turn on tip correct after calibration		   
						   
V1.0.2	
	·	File close error fixed			   
	·	Perimeter routine stops off of part		   
						   
						   
V1.1.0	
	·	Cleanup screenset layout			   
	·	Fixed all routines to work with CSMIO (CSMIO returns x=0, y=0, z=0 on probing miss, while paraport and SmootStepper return actual location data)	   
	·	Added counter feedbackto the perimeter probing screen	   
	·	Corrected diameter mode bore measurement for a backoff error	   
	·	Added second calibration mode (Option 2 - manually center spindle)	   
	·	Added probeActive checks in perimeter routine for safety
	   
						   
V1.1.1	
	·	Correction to 'post' routine and depth value	   
	·	Allow negative probe tip correction values in calibration table (for option 2 routine)	 


V1.1.2
 
	·	Record Z postions in DXF, basic and perimeter routines	   
	·	Warn of 'zero mode on' when recording	 , turn off DXF temporarily  
	·	Updated Calibration Option 2 (find center and set x/y offset)	   
	·	Add offsets to all probing functions	   
	·	Update setZ (hit code, change ZDRO set to center of ball)	   
	·	update touchz (change surface to bottom of ball)	   
	·	Added Z up/down buttons for manual control	   
	·	Constrain slope change on perimimeter routine added	   
	·	Added rapid FRO control 	   
	·	Fix tip correct lookup error (negative angles)	   
	·	Fixed perimeter DXF write of interpolated Corners	   
	·	Altered calibration routines to discard prior data.
	·	General screenset cleanup
	·	Manual updated and improved


V1.1.3 
 
	·	Added auto corner find/G68 rotation 	
	·	Added 'menu' page, and TAB flyout menu page.
	·	fix 'version' reading to c: specific
	·	add Mach3 revision check/warning
	·	made recorded file open/appending relative to Mach path (not hard to C:\),                    		works with non-standard Mach3 installs now.
	·	added 20ms delay in license checking
	.	Added 'gcode' run page, so user can script their own probe routines-info on how to do it coming.
	.	Cleaned up screenset/resized to better fit 1024x768 monitors
	.	Added X/Z probing routing page (prelim version)


V1.1.4
	.	Fix clearance moves in post routine
	.	Add check for 'hit' and mis tolerance in post routine
	.	Fix issue with negative z surface for post and ridge routines
	.	Added info for how to do Gcode calls to probing in manual, and example files



