**PTZ/Network Camera Firmware Version:** **V5.7.3**

**Release Note**

**(2022-01-25)**

|  |  |  |
| --- | --- | --- |
| **Firmware****Basic Information** | Firmware Version: | IPDE\_L\_H8\_EN\_STD\_5.7.3\_211229IPDE\_L\_H8\_EN\_NEU\_5.7.3\_211229 |

**Camera Features**

1. **New Features**

N/A

1. **Improved Features**
* TLS1.1 is OFF by default
* Max resolution of face capture picture is 1920\*1080P
1. **Leftover Issues**

N/A

**Customer Impact and Recommended Action**

This update refers to function/compatibility improvement and will take effect automatically after the Date of Change. We are very sorry for any inconvenience of use-habit changes caused by this action.

For any questions and request for this firmware, please contact our local technical support team.

***Remarks:***

* Hikvision reserves the right to change, alter or withdraw the above notification without prior notice.
* Product design and specifications are subject to change without prior notice.
* The Hikvision firmware may contain errors known as errata which may cause the product to deviate from published specifications. Current characterized errata are available on request.
* Hikvision is not liable for any typing or printing errors.

Hikvision Digital Technology CO., Ltd.

No. 555 Qianmo Road, Binjiang District, Hangzhou 310051, China

Tel: +86-571-8807-5998

FAX: +86-571-8993-5635

Email: overseabusiness@hikvision.com

|  |
| --- |
| **Supported Product List** |
| **Product Category** | **Model Number** |
| DE Series | DS-2DE4215IW-DE(T5) |
| DE Series | DS-2DE4225IW-DE(T5) |
| DE Series | DS-2DE4415IW-DE(T5) |
| DE Series | DS-2DE4425IW-DE(T5) |
| DE Series | DS-2DE5225W-AE(3)(T5) |
| DE Series | DS-2DE5232W-AE(3)(T5) |
| DE Series | DS-2DE5425IW-AE(T5) |
| DE Series | DS-2DE7A225IW-AEB(T5) |
| DE Series | DS-2DE7A232IW-AEB(T5) |
| DE Series | DS-2DE7A425IW-AEB(T5) |
| DE Series | DS-2DE7A825IW-AEB(T5) |

*Note: Models in red font are newly released models.*