**Network Camera Firmware Version:** **V5.5.114**

**Release Note(Internal)**

**(2021-05-24)**

|  |  |  |
| --- | --- | --- |
| **Firmware**  **Basic Information** | Firmware Version: | V5.5.114 build210428 |

**2xx3G2, 2xx6G2, 2xx7G2, 3xx3G2, 3xx6G2, 3xx7G2 Camera V5.5.114 Features**

1. **New Features**

* Newly release 2x47G2 models which support separate flash alarm linkage.

1. **Improved Features**

* Optimize the image effect of 2xx3G2 devices.
* Solve the issue that the device cannot be started with a low probability after upgrading to V5.5.113 version.
* Optimize the problem of obvious abnormal vertical lines on the image in a jittery environment.

1. **Leftover Issues**

* This version does not support 2x6xG2, 2x8xG2, 3x6xG2 and 3x8xG2 models upgrading.
* Products that do not support audio output, abnormally support custom voice configuration on Hik-Connect.
* The audio freezes when playing back a third-stream video file. At this time, you can skip a short segment of the video, and the audio can be played normally.
* When the 3x2x model is set to a high frame rate, after switching from the Monitoring mode to the Smart Event mode or Face Capture mode, the interface displays 25 frames, and the actual is 50 frames. Reconfigure the I frame rate parameters to return to normal.

**Customer Impact and Recommended Action**

This update refers to function/compatibility improvement and will take effect automatically after the Date of Change. We are very sorry for any inconvenience of use-habit changes caused by this action.

For any questions and request for this firmware, please contact our local technical support team.

***Remarks:***

* Hikvision reserves the right to change, alter or withdraw the above notification without prior notice.
* Product design and specifications are subject to change without prior notice.
* The Hikvision firmware may contain errors known as errata which may cause the product to deviate from published specifications. Current characterized errata are available on request.
* Hikvision is not liable for any typing or printing errors.

Hikvision Digital Technology CO., Ltd.

No. 555 Qianmo Road, Binjiang District, Hangzhou 310051, China

Tel: +86-571-8807-5998

FAX: +86-571-8993-5635

Email: overseabusiness@hikvision.com

|  |  |
| --- | --- |
| **Supported Product List (1x83G0, 2xx3G2, 2xx6G2(C), 2xx7G2(C), 3xx3G2, 3xx6G2(C), 3xx7G2(C) Series)** | |
| **Product Category** | **Model Number** |
| 1 Series | DS-2CD1083G0-I(U)(F) |
| 1 Series | DS-2CD1183G0-I(U)(F) |
| 1 Series | DS-2CD1383G0-I(U)(F) |
| Pro Series | DS-2CD2023G2-I(U) |
| Pro Series | DS-2CD2043G2-I(U) |
| Pro Series | DS-2CD2123G2-I(S) |
| Pro Series | DS-2CD2123G2-IU |
| Pro Series | DS-2CD2143G2-I(S) |
| Pro Series | DS-2CD2143G2-IU |
| Pro Series | DS-2CD2323G2-I(U) |
| Pro Series | DS-2CD2343G2-I(U) |
| Pro Series | DS-2CD2423G2-I |
| Pro Series | DS-2CD2443G2-I |
| Pro Series | DS-2CD2623G2-IZS |
| Pro Series | DS-2CD2643G2-IZS |
| Pro Series | DS-2CD2723G2-IZS |
| Pro Series | DS-2CD2743G2-IZS |
| Pro Series | DS-2CD2H23G2-IZS |
| Pro Series | DS-2CD2H43G2-IZS |
| Pro Series | DS-2CD2T23G2-2I/4I |
| Pro Series | DS-2CD2T43G2-2I/4I |
| Pro/2 Series with AcuSense | DS-2CD2026G2-I(U)(C) |
| Pro/2 Series with AcuSense | DS-2CD2026G2-IU/SL(C) |
| Pro/2 Series with AcuSense | DS-2CD2046G2-I(U)(C) |
| Pro/2 Series with AcuSense | DS-2CD2046G2-IU/SL(C) |
| Pro/2 Series with AcuSense | DS-2CD2126G2-I(SU)(C) |
| Pro/2 Series with AcuSense | DS-2CD2146G2-I(SU)(C) |
| Pro/2 Series with AcuSense | DS-2CD2326G2-I(U)(C) |
| Pro/2 Series with AcuSense | DS-2CD2326G2-ISU/SL(C) |
| Pro/2 Series with AcuSense | DS-2CD2346G2-I(U)(C) |
| Pro/2 Series with AcuSense | DS-2CD2346G2-ISU/SL(C) |
| Pro/2 Series with AcuSense | DS-2CD2426G2-I(C) |
| Pro/2 Series with AcuSense | DS-2CD2446G2-I(C) |
| Pro/2 Series with AcuSense | DS-2CD2626G2(T)-IZS(C) |
| Pro/2 Series with AcuSense | DS-2CD2626G2-IZSU/SL(C) |
| Pro/2 Series with AcuSense | DS-2CD2646G2(T)-IZS(C) |
| Pro/2 Series with AcuSense | DS-2CD2646G2-IZSU/SL(C) |
| Pro/2 Series with AcuSense | DS-2CD2726G2(T)-IZS(C) |
| Pro/2 Series with AcuSense | DS-2CD2746G2(T)-IZS(C) |
| Pro/2 Series with AcuSense | DS-2CD2H26G2(T)-IZS(C) |
| Pro/2 Series with AcuSense | DS-2CD2H46G2(T)-IZS(C) |
| Pro/2 Series with AcuSense | DS-2CD2T26G2-2I/4I(C) |
| Pro/2 Series with AcuSense | DS-2CD2T26G2-ISU/SL(C) |
| Pro/2 Series with AcuSense | DS-2CD2T46G2-2I/4I(C) |
| Pro/2 Series with AcuSense | DS-2CD2T46G2-ISU/SL(C) |
| Pro/2 Series with ColorVu | DS-2CD2027G2-L(U)(C) |
| Pro/2 Series with ColorVu | DS-2CD2047G2-L(U)(C) |
| Pro/2 Series with ColorVu | DS-2CD2047G2-LU/SL(C) |
| Pro/2 Series with ColorVu | DS-2CD2127G2(-SU)(C) |
| Pro/2 Series with ColorVu | DS-2CD2147G2(-SU)(C) |
| Pro/2 Series with ColorVu | DS-2CD2327G2-L(U)(C) |
| Pro/2 Series with ColorVu | DS-2CD2347G2-L(U)(C) |
| Pro/2 Series with ColorVu | DS-2CD2347G2-LSU/SL(C) |
| Pro/2 Series with ColorVu | DS-2CD2647G2-LZS(C) |
| Pro/2 Series with ColorVu | DS-2CD2747G2-LZS(C) |
| Pro/2 Series with ColorVu | DS-2CD2T27G2-L(C) |
| Pro/2 Series with ColorVu | DS-2CD2T47G2-L(C) |
| Pro/2 Series with ColorVu | DS-2CD2T47G2-LSU/SL(C) |
| Pro/3 Series with AcuSense | DS-2CD3026G2-IS(C) |
| Pro/3 Series with AcuSense | DS-2CD3026G2-IU/SL(C) |
| Pro/3 Series with AcuSense | DS-2CD3056G2-IS(C) |
| Pro/3 Series with AcuSense | DS-2CD3056G2-IU/SL(C) |
| Pro/3 Series with AcuSense | DS-2CD3126G2-IS(U)(C) |
| Pro/3 Series with AcuSense | DS-2CD3156G2-IS(U)(C) |
| Pro/3 Series with AcuSense | DS-2CD3326G2-IS(U)(C) |
| Pro/3 Series with AcuSense | DS-2CD3326G2-ISU/SL(C) |
| Pro/3 Series with AcuSense | DS-2CD3356G2-IS(U)(C) |
| Pro/3 Series with AcuSense | DS-2CD3356G2-ISU/SL(C) |
| Pro/3 Series with AcuSense | DS-2CD3626G2(T)-IZS(C) |
| Pro/3 Series with AcuSense | DS-2CD3656G2(T)-IZS(C) |
| Pro/3 Series with AcuSense | DS-2CD3726G2(T)-IZS(C) |
| Pro/3 Series with AcuSense | DS-2CD3756G2(T)-IZS(C) |
| Pro/3 Series with AcuSense | DS-2CD3B26G2T-IZHSY(C) |
| Pro/3 Series with AcuSense | DS-2CD3B46G2T-IZHSY(C) |
| Pro/3 Series with AcuSense | DS-2CD3H26G2-IZS(C) |
| Pro/3 Series with AcuSense | DS-2CD3H56G2-IZS(C) |
| Pro/3 Series with AcuSense | DS-2CD3T26G2-4IS(C) |
| Pro/3 Series with AcuSense | DS-2CD3T26G2-ISU/SL(C) |
| Pro/3 Series with AcuSense | DS-2CD3T56G2-4IS(C) |
| Pro/3 Series with AcuSense | DS-2CD3T56G2-ISU/SL(C) |
| Pro/3 Series with ColorVu | DS-2CD3047G2-LS(U)(C) |
| Pro/3 Series with ColorVu | DS-2CD3347G2-LS(U)(C) |
| Pro/3 Series with ColorVu | DS-2CD3647G2-LZS(C) |
| Pro/3 Series with ColorVu | DS-2CD3747G2-LZS(C) |

*Note: Models in red font are newly released models.*