**PTZ DY5&DY7& Explosion-proof Camera Firmware Version:** **V5.7.0**

**Release Note(Internal)**

**(2021-08-20)**

|  |  |  |
| --- | --- | --- |
| **Firmware**  **Basic Information** | Firmware Version: | 5.7.0 |
| SDK Version: | V1.2.0.19 build1210506 |
| iVMS-4200: | V3.4.2.1 build20210105 |
| Hik-Connect: | V2.3.0 build 210704 |

DY5:

IPYT\_H8\_EN\_NEU\_5.7.1\_210714

IPYT\_H8\_EN\_STD\_5.7.1\_210714

DY7:

IPTM\_H8\_EN\_NEU\_5.7.1\_210714

IPTM\_H8\_EN\_STD\_5.7.1\_210714

Explosion-proof DF dome:

IPDE\_EX\_H8\_EN\_NEU\_5.7.1\_210714

IPDE\_EX\_H8\_EN\_STD\_5.7.1\_210714

Explosion-proof DY positioning-system:

IPYT\_EX\_H8\_EN\_NEU\_5.7.1\_210714

IPYT\_EX\_H8\_EN\_STD\_5.7.1\_210714

Explosion-proof Bullet:

IPZEX\_H8\_EN\_NEU\_5.7.1\_210714

IPZEX\_H8\_EN\_STD\_5.7.1\_210714

**Camera Features**

1. **New Features**

* Newly release the below models:

Please refer to the Supported Product List

* New feature release:

(1) DY5, DY7:

Face capture, Smart perimeter event with Auto-tracking

(2) Explosion-proof dome/positioning-system/bullet:

Face capture and comparison, Smart perimeter event with Auto-tracking

*Note: The face library for explosion-proof device supports up to 10000 pictures for 10 libraries and each and total maximum number of library is 10000, storage capacity is 3Gb.*

1. **Improved Features**

N/A

1. **Leftover Issues**

N/A

**Customer Impact and Recommended Action**

This update refers to function/compatibility improvement and will take effect automatically after the Date of Change. We are very sorry for any inconvenience of use-habit changes caused by this action.

For any questions and request for this firmware, please contact our local technical support team.

***Remarks:***

* Hikvision reserves the right to change, alter or withdraw the above notification without prior notice.
* Product design and specifications are subject to change without prior notice.
* The Hikvision firmware may contain errors known as errata which may cause the product to deviate from published specifications. Current characterized errata are available on request.
* Hikvision is not liable for any typing or printing errors.

Hikvision Digital Technology CO., Ltd.

No. 555 Qianmo Road, Binjiang District, Hangzhou 310051, China

Tel: +86-571-8807-5998

FAX: +86-571-8993-5635

Email: overseabusiness@hikvision.com

|  |  |
| --- | --- |
| **Supported Product List** | |
| **Product Category** | **Model Number** |
| DY5 | DS-2DY5225IX-AE(T5)(O-STD&NEU) |
| DY5 | DS-2DY5225IX-DM(T5)(O-STD) |
| DY7 | DS-2DY7236IX-A(T5)（O-STD&NEU） |
| Explosion-proof dome | DS-2DF6223-CX(T5/316L)（O-STD&NEU） |
| Explosion-proof dome | DS-2DF6231-CX(T5/316L)（O-STD&NEU） |
| Explosion-proof dome | DS-2DF6C223-CX(T5/316L)（O-STD&NEU） |
| Explosion-proof DY | DS-2DY9236I-CWX(T5/316L)（O-STD&NEU） |
| Explosion-proof bullet | DS-2DB4223I-CX(T5/316L)（O-STD&NEU） |
| Explosion-proof bullet | DS-2DB4236I-CWX(T5/316L)（O-STD&NEU） |

*Note: Models in red font are newly released models.*