**Secure Module DS-K2M061 V1.0 Release Note**

**(2020-12-11)**

|  |  |  |
| --- | --- | --- |
| Device Model:Controller:DS-K2M061 | Firmware Version | ACS\_DS-K2M061\_M2pro\_GML\_GM\_V1.0.0\_build201024 |
| SDK Version | NA |
| iVMS4200 Version | NA |

**Features**

1. Communicates with the access control terminal via RS-485 to execute the commands from the terminal including open door, close door, normally open and normally closed;
2. Supports fire alarm hardware linkage;
3. Supports tampering alarm;
4. Input/output interface: Exit button × 1, Lock × 1, Door contact × 1, Alarm input × 2; Alarm output × 1; RS485 × 1 and Wiegand × 1; Fire alarm input × 1

***Remarks:***

* Hikvision reserves the right to change, alter or withdraw the above notification without prior notice.
* Product design and specifications are subject to change without prior notice.
* The Hikvision firmware may contain errors known as errata which may cause the product to deviate from published specifications. Current characterized errata are available on request.
* Hikvision is not liable for any typing or printing errors.

Hikvision Digital Technology CO., Ltd.

No. 555 Qianmo Road, Binjiang District, Hangzhou 310051, China

Tel: +86-571-8807-5998

FAX: +86-571-8993-5635

Email: overseabusiness@hikvision.com